# trx-rs v{ver}

trx-rs
trx-client v{ver}
Rig: --
Access Required
Enter passphrase to continue
Initializing (rig)…
Bandwidth kHz
Peak Hold
Floor dB
Contrast 1.0
Scroll to zoom · Ctrl+Scroll to tune · Drag to pan · Drag BW edges to resize
Pinch to zoom · Drag to pan · Drag BW edges to resize
50/50
--
Wavelength
Frequency
Center Frequency
Unit
Step Scale
Mode
Deemp
Audio
Denoise Level
Pilot MO
WFM
Transmit / Power
VFO
SDR settings
Hardware AGC
RF Gain
LNA Gain
Noise Blanker
NB Threshold
Channels / Scheduler
Scheduler is controlling the rig.
Interleaving: --
Signal
--
TX Meters
PWR --
SWR --
TX Limit — units depend on rig (percentage/watts)
Audio
RX80% TX80% SQLOpen
Off
Add Bookmark
Name Category Frequency (Hz) Mode Bandwidth (Hz) Locator
Decoders
APRS AIS FT8 FT4 FT2 WSPR HF APRS
Comment

| Name | Frequency | Mode | BW | Locator | Category | Decoders | Comment | Actions
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---

No bookmarks yet. Click + Add Bookmark to save a frequency.
Showing 0-0 of 0
Page 1 of 1
AIS Decoder
Decodes dual-channel AIS traffic from RX audio using 9.6 kbit/s GMSK and HDLC.
VDES Decoder
Decodes single-channel 100 kHz VDES bursts from SDR IQ using the dedicated VDES path.
APRS Decoder
Decodes APRS packets from RX audio using Bell 202 AFSK (1200 baud).
CW Decoder
Decodes CW (Morse code) from RX audio.
FT8 Decoder
Decodes FT8 messages from RX audio (DIG/USB only, toggle required).
FT4 Decoder
Decodes FT4 messages from RX audio (DIG/USB only, toggle required). 7.5-second slots.
FT2 Decoder
Decodes FT2 messages from RX audio (DIG/USB only, toggle required). 3.75-second slots.
WSPR Decoder
Decodes WSPR messages from RX audio (DIG/USB only, toggle required).
RDS Decoder
Decodes Radio Data System (RDS) metadata from WFM broadcasts (57 kHz subcarrier).
StatusNo signal
Active mode--
PI--
PS--
PTY--
PTY Code--
PTYN--
TP--
TA--
Audio--
Stereo--
Compressed--
Artificial Head--
Dynamic PTY--
AF--
RadioText--
Raw JSON (last spectrum frame)

    --

Waiting for server decode
Channels A 161.975 MHz · B 162.025 MHz
Tracked 0 vessels
Latest No traffic yet
Waiting for server decode
Channel 100 kHz centered on tuned frequency
Frames 0 bursts
Latest No traffic yet
Waiting for server decode
Frames 0 total
Visible 0 shown
Latest No packets yet
Waiting for server decode
Frames 0 total
Visible 0 shown
Latest No packets yet
Waiting for server decode Next slot --s
Time SNR DT RF Message
Showing up to 200 most recent decodes. Full history is available on the Map tab.
Waiting for server decode Next slot --s
Time SNR DT RF Message
Showing up to 200 most recent decodes. Full history is available on the Map tab.
Waiting for server decode Next slot --s
Time SNR DT RF Message
Showing up to 200 most recent decodes. Full history is available on the Map tab.
Waiting for server decode Next slot --:--
Time SNR DT RF Message
Waiting for server decode
Auto WPM + Tone WPM Tone (Hz)
CW Audio Tone Picker --
Filter by
Show
Rig
Search
History
Paths
TRX paths on popup, directed decode paths when target locator is known
Longest decode paths
Top 5 directed decode paths in the current map view
Strongest decoded signal
Top 5 strongest signals in the current map history
Weakest decoded signal
Top 5 weakest signals in the current map history
Mode
Grayline Settings
Latitude (°) Longitude (°) Transition window (min)
Dawn bookmark
Day bookmark
Dusk bookmark
Night bookmark
Time Span Entries (UTC)
Interleave time (min) When multiple entries overlap, spend this many minutes at each before cycling. Leave blank to disable.

Start | End | Center freq | Primary bookmark | Extra channels | Label | Interleave (min) |
--- | --- | --- | --- | --- | --- | --- | ---

Add Entry
Start (UTC) End (UTC) Center freq (Hz, SDR) Primary bookmark
Extra channels (virtual)
Label (optional) Interleave (min, optional)
Last Activity
No activity yet.
Configuration
Background decode Enable hidden background decoder channels
Bookmark
Runtime Status
No background decode bookmarks configured.
Full Decode History
These buttons clear the server-side decode history and reset the corresponding decoder state.
Authenticated as: --

Server version | --
Server address | --
Server callsign | --
Rig | --
Active rig | --
Available rigs | --
Rig connection | --
Supported modes | --
VFOs | --
Rigctl endpoint | --
Rigctl clients | --
PSK Reporter | --
APRS-IS | --
Client version | {pkg} v{ver}
Connected clients | --

Connection lost
Retrying…
Loading decode history…
Preparing recent decodes for the UI