# trx-rs v{ver}

trx-rs
Rig: --
Access Required
Enter passphrase to continue
Initializing (rig)…
Bandwidth kHz
Peak Hold
Floor dB
Scroll to zoom · Ctrl+Scroll to tune · Drag to pan · Drag BW edges to resize
Pinch to zoom · Drag to pan · Drag BW edges to resize
--
Wavelength
Frequency
Center Frequency
Unit
Step Scale
Mode
Deemp
Audio
Denoise Level
RF Gain
Pilot MO
WFM
Transmit / Power
VFO
Signal
--
TX Meters
PWR --
SWR --
TX Limit — units depend on rig (percentage/watts)
Audio
RX80% TX80%
Off
Add Bookmark
Name Category Frequency (Hz) Mode Bandwidth (Hz)
Decoders
FT8 WSPR
Comment

Name | Frequency | Mode | BW | Category | Decoders | Comment | Actions
--- | --- | --- | --- | --- | --- | --- | ---

No bookmarks yet. Click + Add Bookmark to save a frequency.
AIS Decoder
Decodes dual-channel AIS traffic from RX audio using 9.6 kbit/s GMSK and HDLC.
VDES Decoder
Decodes single-channel 100 kHz VDES bursts from SDR IQ using the dedicated VDES path.
APRS Decoder
Decodes APRS packets from RX audio using Bell 202 AFSK (1200 baud).
CW Decoder
Decodes CW (Morse code) from RX audio.
FT8 Decoder
Decodes FT8 messages from RX audio (DIG/USB only, toggle required).
WSPR Decoder
Decodes WSPR messages from RX audio (DIG/USB only, toggle required).
RDS Decoder
Decodes Radio Data System (RDS) metadata from WFM broadcasts (57 kHz subcarrier).
StatusNo signal
Active mode--
PI--
PS--
PTY--
PTY Code--
PTYN--
TP--
TA--
Audio--
Stereo--
Compressed--
Artificial Head--
Dynamic PTY--
AF--
RadioText--
Raw JSON (last spectrum frame)

    --

Waiting for server decode
Channels A 161.975 MHz · B 162.025 MHz
Tracked 0 vessels
Latest No traffic yet
Waiting for server decode
Channel 100 kHz centered on tuned frequency
Frames 0 bursts
Latest No traffic yet
Waiting for server decode
Frames 0 total
Visible 0 shown
Latest No packets yet
Waiting for server decode Next slot --s
Time SNR DT RF Message
Waiting for server decode Next slot --:--
Time SNR DT RF Message
Waiting for server decode
Auto WPM WPM Tone (Hz)
CW Tone From Selected BW --
AIS VDES APRS FT8 WSPR
Authenticated as: --

Server version | --
Server address | --
Server callsign | --
Rig | --
Active rig | --
Available rigs | --
Rig connection | --
Supported modes | --
VFOs | --
Rigctl endpoint | --
Rigctl clients | --
PSK Reporter | --
Client version | {pkg} v{ver}
Connected clients | --