<div align="center">
  <img src="assets/trx-logo.png" alt="trx-rs logo" width="25%" />
</div>

# trx-rs

A modular transceiver control stack with configurable backends and frontends. The rig task is driven by controller components (state machine, handlers, and policies) with configurable polling and retry behavior via the `[behavior]` section in the config file.

**Note**: This is a live project with evolving APIs. Please report issues and feature requests.

Configuration reference: see `CONFIGURATION.md` for all server/client options and defaults.

## Configuration Files

`trx-server` and `trx-client` read configuration from a shared `trx-rs.toml`.

- Default search order for each app:
  current directory, then `~/.config/trx-rs`, then `/etc/trx-rs`
- At each location, the loader checks:
  `trx-rs.toml` and reads the `[trx-server]` or `[trx-client]` section
- Config file name:
  `trx-rs.toml`
- `--config <FILE>` loads an explicit config file path and reads the matching `[trx-server]` or `[trx-client]` section from that file.
- `--print-config` prints an example combined config block suitable for `trx-rs.toml`.

See `trx-rs.toml.example` for a complete combined example.

## Supported backends

- Yaesu FT-817 (feature-gated crate `trx-backend-ft817`)
- Planned: other rigs I own; contributions and reports are welcome.

## Frontends

- HTTP status/control frontend (`trx-frontend-http`)
- JSON TCP control frontend (`trx-frontend-http-json`)
- rigctl-compatible TCP frontend (`trx-frontend-rigctl`, listens on 127.0.0.1:4532)

## HTTP Frontend Authentication

The HTTP frontend supports optional passphrase-based authentication with two roles:

- **rx**: Read-only access to status, events, decode history, and audio streams
- **control**: Full access including transmit control (TX/PTT) and power toggling

Authentication is disabled by default. When enabled, users must log in via a passphrase before accessing the web UI. Sessions are managed server-side with configurable time-to-live and cookie security settings.

### Configuration

Enable authentication under `[trx-client.frontends.http.auth]` in `trx-rs.toml`.

```toml
[trx-client.frontends.http.auth]
enabled = true
rx_passphrase = "read-only-secret"
control_passphrase = "full-control-secret"
session_ttl_min = 480          # 8 hours
cookie_secure = false          # Set to true for HTTPS
cookie_same_site = "Lax"
```

### Security Considerations

- **Local/LAN use**: Default settings are safe for 127.0.0.1 or trusted local networks.
- **Remote access**: For internet-exposed deployments:
  - Deploy behind HTTPS (reverse proxy or TLS termination)
  - Set `cookie_secure = true`
  - Use strong passphrases (random, 16+ chars)
  - Consider firewall rules and network segmentation
- **Passphrase storage**: Passphrases are stored in plaintext in the config file. Protect the config file with appropriate file permissions.
- **No rate limiting**: The current implementation does not include login rate limiting. For high-security scenarios, deploy behind a reverse proxy with rate limiting.

### Architecture

- **Sessions**: In-memory, expire after configured TTL (default 8 hours)
- **Cookies**: HttpOnly, configurable Secure and SameSite attributes
- **Route protection**: Middleware validates session on protected endpoints; public routes (static assets, login) are always accessible
- **TX/PTT gating**: Control-only endpoints return 404 to rx-authenticated users (when `tx_access_control_enabled=true`)

## Audio streaming

Bidirectional Opus audio streaming between server, client, and browser.

- **Server** captures audio from a configured input device (cpal), encodes to Opus, and streams over a dedicated TCP connection (default port 4533). TX audio received from clients is decoded and played back.
- **Client** connects to the server's audio TCP port and relays Opus frames to/from the HTTP frontend via a WebSocket at `/audio`.
- **Browser** connects to the `/audio` WebSocket, decodes Opus via WebCodecs `AudioDecoder`, and plays RX audio. TX audio is captured via `getUserMedia` and encoded with WebCodecs `AudioEncoder`.

Enable with `[audio] enabled = true` in the server config and `[frontends.audio] enabled = true` in the client config.

## Dependencies

### System libraries

The following system libraries are required at build time:

| Library | Purpose | Install |
|---------|---------|---------|
| **libopus** | Opus audio codec encoding/decoding | `zb install opus` (or your system package manager) |
| **libsoapysdr** | Required for SoapySDR-based SDR backends | `zb install soapysdr` (or your system package manager) |
| **cmake** | Required by the `audiopus_sys` build script if libopus is not found via pkg-config | `zb install cmake` |
| **pkg-config** / **pkgconf** | Locates system libopus during build | `zb install pkgconf` |
| **Core Audio** (macOS) / **ALSA** (Linux) | Audio device access via cpal | Provided by the OS (macOS) or `alsa-lib-dev` (Linux) |

## Plugin discovery

`trx-server` and `trx-client` can load shared-library plugins that register backends/frontends
via a `trx_register` entrypoint. Search paths:

- `./plugins`
- `~/.config/trx-rs/plugins`
- `TRX_PLUGIN_DIRS` (path-separated)

Example plugin: `examples/trx-plugin-example`

## License

This project is licensed under the BSD-2-Clause license. See `LICENSES/` for bundled third-party license files.
